EDIBON

Edition:ED01/26
Date:June/2026
T/KIT4
REFRIGERATION MAINTENANCE TOOLS KIT

TENDER SPECIFICATIONS
Countersink.

Tube bender.

1/4” copper tube and 3/8” copper tube.

Open-ended spanners:

    Metric 10 x 11 mm.

    Metric 12 x 13 mm.

    Metric 16 x 17 mm.

    Metric 18 x 19 mm.

    Metric 20 x 22 mm.

10” adjustable wrench.

“Flat-head” screwdriver and “star-head” screwdriver.

Voltage tester screwdriver.

Cutter.

Scissors.

Battery-operated digital multimeter for direct and alternating current.

Battery-operated refrigerant gas leak detector for R-513a refrigerant.

Toolbox made of plastic.

- Dimensions: 70 x 35 x 40 mm approx. (2.76 x 1.38 x 1.57 inches approx.) - Weight: 35 kg approx. (77.16 pounds approx.)
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